%%
%% Sample TeX file for the HRMS Dijon 2023 abstracts
%% 
%% Lines (or parts of) beginning with at least one '%' are comments 
%% and are silently ignored by LaTeX
%%
%% Codings beginning with \ are LaTeX macros, or commands.
%% They are used to tell the LaTeX parser how to format the document.
%% All the macros below are mandatory.
%%
%% Various informations about latex may be found at
%%
%%   http://en.wikibooks.org/wiki/LaTeX
%%
%% *-----------------------------------------------------------------------------------------*
\documentclass[11pt]{article}

\usepackage{hrms}  %% Page settings, style ... for the HRMS abstract book.

%% *-----------------------------------------------------------------------------------------*

\title{ON-SITE $\&$ REAL TIME THz MONITORING OF GASEOUS EMISSION FROM A WASTE RECOVERY CENTER}

%% Note that \author and \address macros must be paired.
%% The names of authors must also appear IN CAPITALS.
%% The name(s) of author(s) presenting the work is(are) usually underlined.

\author{ \FirstName J. \LastName DECKER, \FirstName F. \LastName HINDLE, \FirstName E. \LastName FERTEIN, \FirstName N. \LastName HOUZEL, \underline{\FirstName G. \LastName MOURET}, \underline{\FirstName A. \LastName CUISSET}}
\address{Laboratoire de Physico-Chimie de l'Atmosph\`ere, UR4493, Universit\'e du Littoral C\^ote d'Opale, Dunkerque, France}
\author{ \FirstName F. \LastName CAZIER}
\address{Centre Commun de Mesures, Universit\'e du Littoral C\^ote d'Opale, Dunkerque, France}
\author{\FirstName J. \LastName DUMONT}
\address{Paprec Energies 59, Paprec, Dunkerque, France}
%% The \FirstName and \LastName macros are mandatory for each author
%% to make sure that the author index is properly auto-generated.
%% Otherwise, these macros do nothing in particular.

%% Add or remove \author and \address pair(s) below to suite your needs


%% *-----------------------------------------------------------------------------------------*

%% Place below other \usepackage{ ... }, if you need other packages.
%% See http://www.tug.org/texlive/doc.html for a description of available packages.

%% The macros below will change the page head and foot.
%% Please, do not modify the content of the \fancyhead macro nor the \fancyfoot line.
\usepackage{fancyhdr}
\pagestyle{fancy}
\fancyhead[C]{{\footnotesize \textit{HRMS, 28th Colloquium, Dijon, France,
  Aug. 28 - Sept. 1, 2023}}}
\fancyfoot[C]{}
\renewcommand{\headrulewidth}{0.6pt}
\renewcommand{\footrulewidth}{0.6pt}

%% The hyperref package allows to include hyperlinks in a document.
%% See the instructions for abstract submission for more details.
%% WARNING: Make sure that this package comes LAST since it re-defines many LaTeX macros.
\usepackage[colorlinks=true,urlcolor=blue,linkcolor=blue,citecolor=blue]{hyperref}
\voffset -.65 cm

%% *-----------------------------------------------------------------------------------------*

\category {9,15}
\begin{document}

\maketitle  %% This will also build the list of author(s) and addresse(s).

%% Index macro(s): see the abstract samples and the instructions
%% Remove the %% to account for the index item(s)
%% \index{Item1}
%% \index{Item2}

%% Place the body of your abstract below.

The Dunkirk waste recovery center continuously treats all of the urban community's household waste by converting it into electrical and thermal energy through incineration. These activities are carried out with a controlled environmental impact, based on continuous improvement. The TeraWaste project explores the potential of high-resolution TeraHertz spectroscopy for continuous monitoring of gaseous emissions by developing an on-site diagnostic unit. The selectivity and the ability to detect in scattering media make it a relevant alternative to current multi-compounds monitoring solutions. In this context, we have dedicated a sub-millimeter wave source based on a frequency multiplication chain for industrial monitoring applications.\footnote{\href{http://dx.doi.org/10.1109/JSEN.2012.2227055}{doi:10.1109/JSEN.2012.2227055}, G. Mouret \textit{et al.} Versatile Sub-THz Spectrometer for Trace Gas Analysis, IEEE Sens. J., 13(1), 133-138 (2013).} The spectrometer has been characterized by determining the limits of detection of the regulated polar pollutants. Rotational spectroscopy measurements on real process and emission gases, sampled and analyzed off-line as well as in real time on-site, were performed over several hours and compared with standard reference methods and the certified continuous measurement system. Using an adapted preconcentration/thermal desorption setup\footnote{\href{http://dx.doi.org/10.1109/JSEN.2012.2195487}{doi:10.1109/JSEN.2012.2195487}, C.~F. Neese \textit{et al.} Compact Submillimeter/Terahertz Gas Sensor With Efficient Gas Collection, Preconcentration, and ppt Sensitivity, IEEE Sens. J., 12(8), 2565-2574 (2012).}$^,$\footnote{\href{http://dx.doi.org/10.3390/s19122719}{doi:10.3390/s19122719}, N. Rothbart \textit{et al.} Analysis of Human Breath by Millimeter-Wave/Terahertz Spectroscopy, Sensors, 19(12), 2719 (2019).}, a quantified multi-species mapping, extended to the various polar compounds absorbing the sub-mm waves of the plant's gaseous emissions, in particular VOCs by discriminating them, will enable the operator to better meet current standards and anticipate potential evolution in the regulations.



\end{document}
