%%
%% Sample TeX file for the HRMS Dijon 2023 abstracts
%% 
%% Lines (or parts of) beginning with at least one '%' are comments 
%% and are silently ignored by LaTeX
%%
%% Codings beginning with \ are LaTeX macros, or commands.
%% They are used to tell the LaTeX parser how to format the document.
%% All the macros below are mandatory.
%%
%% Various informations about latex may be found at
%%
%%   http://en.wikibooks.org/wiki/LaTeX
%%
%% *-----------------------------------------------------------------------------------------*
\documentclass[11pt]{article}

\usepackage{hrms}  %% Page settings, style ... for the HRMS abstract book.

%% *-----------------------------------------------------------------------------------------*

\title{IMPROVEMENTS OF THE FANTASIO EXPERIMENTAL SETUP}

%% Note that \author and \address macros must be paired.
%% The names of authors must also appear IN CAPITALS.
%% The name(s) of author(s) presenting the work is(are) usually underlined.
\author{\underline{\FirstName A.S. \LastName BOGOMOLOV}, \FirstName R. \LastName GLORIEUX, \FirstName T. \LastName CORBO}
\address{Institute of Condensed Matter and Nanosciences,
Universit\'e catholique de Louvain, Chemin du cyclotron, 2, 1348, Louvain-la-Neuve, Belgium}
%% The \FirstName and \LastName macros are mandatory for each author
%% to make sure that the author index is properly auto-generated.
%% Otherwise, these macros do nothing in particular.
%% Add or remove \author and \address pair(s) below to suite your needs
\author{\FirstName M. \LastName HERMAN}
\address{Spectroscopy, Quantum Chemistry and Atmospheric Remote Sensing, Facult\'e des Sciences, Universit\'e libre de Bruxelles, 50 ave. F-D Roosevelt, B-1050, Brussels, Belgium}
\author{\FirstName C. \LastName LAUZIN}
\address{Institute of Condensed Matter and Nanosciences,
Universit\'e catholique de Louvain, Chemin du cyclotron, 2, 1348, Louvain-la-Neuve, Belgium}
%% *-----------------------------------------------------------------------------------------*

%% Place below other \usepackage{ ... }, if you need other packages.
%% See http://www.tug.org/texlive/doc.html for a description of available packages.

%% The macros below will change the page head and foot.
%% Please, do not modify the content of the \fancyhead macro nor the \fancyfoot line.
\usepackage{fancyhdr}
\pagestyle{fancy}
\fancyhead[C]{{\footnotesize \textit{HRMS, 28th Colloquium, Dijon, France,
  Aug. 28 - Sept. 1, 2023}}}
\fancyfoot[C]{}
\renewcommand{\headrulewidth}{0.6pt}
\renewcommand{\footrulewidth}{0.6pt}

%% The hyperref package allows to include hyperlinks in a document.
%% See the instructions for abstract submission for more details.
%% WARNING: Make sure that this package comes LAST since it re-defines many LaTeX macros.
\usepackage[colorlinks=true,urlcolor=blue,linkcolor=blue,citecolor=blue]{hyperref}
\voffset -.65 cm

%% *-----------------------------------------------------------------------------------------*

\category {3,5}
\begin{document}

\maketitle  %% This will also build the list of author(s) and addresse(s).

%% Index macro(s): see the abstract samples and the instructions
%% Remove the %% to account for the index item(s)
%% \index{Item1}
%% \index{Item2}

%% Place the body of your abstract below.
The FANTASIO\footnote{\href{http://dx.doi.org/10.1080/00268970601063820}{doi:10.1080/00268970601063820}, M. Herman, K. Didriche, D. Hurtmans, B. Kizil, P. Macko, A. Rizopoulos, P. Van Poucke, {\it Molecular Physics\/}, 
105:5-7, 815--823 (2007).\label{HQ}} is an experimental setup for measuring highly resolved rovibrational spectra of molecules and van der Waals complexes formed in a supersonic expansion. The continuous wave cavity ringdown spectrometer is used for probing the species in the near IR region (\(\sim \)1.4 \(\mu \)m, 0.9 eV). A pulsed slit nozzle is used to increase the interaction path between the laser and the molecular beam. In the present work, I will show the last improvements of the slit nozzle including its new design and the profile of the new slit jaws. The valve can produce expansion from the slit nozzle with a length of up to 80 mm. This provides really intense molecular beam with homogeneous density and temperature distributions along the slit. This new design will be compared with our previous valve based on a 30 mm long slit and Parker series 9 valve with a multichannel bloc\footnote{\href{http://dx.doi.org/10.11575/PRISM/26361}{doi:10.11575/PRISM/26361}, J. Norooz Oliaee, 
Doctoral thesis, University of Calgary,
Calgary, Canada.\label{HQ}}.

Consequently, of the increase of signal-to-noise ratio new rovibrational bands of H$_{2}$O-Ar in the 2OH stretching overtone range were observed and will be presented.

\end{document}
