%%
%% Sample TeX file for the HRMS Dijon 2023 abstracts
%% 
%% Lines (or parts of) beginning with at least one '%' are comments 
%% and are silently ignored by LaTeX
%%
%% Codings beginning with \ are LaTeX macros, or commands.
%% They are used to tell the LaTeX parser how to format the document.
%% All the macros below are mandatory.
%%
%% Various informations about latex may be found at
%%
%%   http://en.wikibooks.org/wiki/LaTeX
%%
\begin{filecontents}{FigEx02.eps}
%!PS-Adobe-3.0 EPSF-3.0

    (body of the PostScript file suppressed)

%%EOF
\end{filecontents}

%% *-----------------------------------------------------------------------------------------*

\documentclass[11pt]{article}

\usepackage{hrms}  %% Page settings, style ... for the HRMS abstract book.
\usepackage{graphicx,amssymb,amsmath}

%% *-----------------------------------------------------------------------------------------*

\title{IFLEX-AGILE: A COMMERCIAL CW-OPO FOR SPECTROSCOPIC APPLICATIONS}

%% Note that \author and \address macros must be paired.
%% The names of authors must also appear IN CAPITALS.
%% The name(s) of author(s) presenting the work is(are) usually underlined.

\author{\FirstName B. \LastName PILLES,
  \FirstName D. \LastName WITSCH and
  \underline{\FirstName F. \LastName MUELLER}}
\address{EXCELITAS TECHNOLOGIES, 85622 Feldkirchen (Munich), Germany, www.excelitas.com}

%% The \FirstName and \LastName macros are mandatory for each author
%% to make sure that the author index is properly auto-generated.
%% Otherwise, these macros do nothing in particular.

%% Add or remove \author and \address pair(s) below to suite your needs


%% *-----------------------------------------------------------------------------------------*

%% Place below other \usepackage{ ... }, if you need other packages.
%% See http://www.tug.org/texlive/doc.html for a description of available packages.

%% The macros below will change the page head and foot.
%% Please, do not modify the content of the \fancyhead macro nor the \fancyfoot line.
\usepackage{fancyhdr}
\pagestyle{fancy}
\fancyhead[C]{{\footnotesize \textit{HRMS, 28th Colloquium, Dijon, France,
  Aug. 28 - Sept. 1, 2023}}}
\fancyfoot[C]{}
\renewcommand{\headrulewidth}{0.6pt}
\renewcommand{\footrulewidth}{0.6pt}

%% The hyperref package allows to include hyperlinks in a document.
%% See the instructions for abstract submission for more details.
%% WARNING: Make sure that this package comes LAST since it re-defines many LaTeX macros.
\usepackage[colorlinks=true,urlcolor=blue,linkcolor=blue,citecolor=blue]{hyperref}
\voffset -.65 cm

%% *-----------------------------------------------------------------------------------------*

\category {UNKNOWN}
\begin{document}

\maketitle  %% This will also build the list of author(s) and addresse(s).

%% Index macro(s): see the abstract samples and the instructions
%% Remove the %% to account for the index item(s)
%% \index{Item1}
%% \index{Item2}

%% Place the body of your abstract below.

Excelitas Technologies Corp. is a photonics technology leader focused on delivering innovative, 
high-performance, market-driven solutions to meet the lighting, optronics, detection and optical technology needs of our OEM customers. 

With the Excelitas brand LINOS being the first company worldwide ever offering cw-OPOs commercially since 1999, the history is continued with the present iFLEX-Agile series. 
Ideal for a variety of applications in mass spectrometry, material testing, trace-gas sensing, spectroscopy, and metrology, 
this compact instrument allows fine-tuning of specific wavelengths from NIR to MIR, having high-quality output beams of high intensity. 
Fully controlled via USB computer interface, iFLEX-Agile enables rapid and reproducible settings of any desired wavelength 
from 1480 up to 1950nm and from 2400 up to 3800nm with output powers exceeding 1W in its basic configuration, and without any need to change optics or modules. 
iFLEX-Agile emission linewidths can vary from 200GHz to below 1MHz depending on its configuration. The modular concept allows modification of wavelength tuning range, 
emission linewidths and output power levels to cost-efficiently meet the custom requirements for specific applications.

The authors acknowledge the support by Claudia Gabler, Georg Koch (technical design) and Tatjana Brill (marketing).

Link to product: https://www.excelitas.com/product/iflex-agile-cw-optical-parametric-oscillator


\end{document}
